SECURITY SYSTEM QUICK REFERENCE GUIDE

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO ARM ENTIRE SYSTEM - BOTH INTERIOR AND PERIMETER**

• Close all windows and doors (the green Ready light will turn ON)

• Press and hold (Away) for 2 seconds (the keypad will beep rapidly

5 times and the red Armed light will turn ON)

• Exit premises before the delay time expires

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO DISARM SYSTEM WHEN YOU RETURN**

. When you enter through the door, the keypad will emit a steady warning tone

• Enter your 4-digit Master Code or User Code (the armed light will turn OFF)

• If you make an error, press # and enter the 4-digit code again

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO ARM PERIMETER OF BUILDING AND STILL MOVE FREELY INSIDE**

• Press and hold (Stay) for 2 seconds

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO ARM SYSTEM WITH DOOR OR WINDOW OPEN**

• Press \* 1 while disarmed

• The Bypass light will flash

• Scroll to zone that you want to bypass

• To exit the Bypass function press # twice

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO SILENCE ALARM**

• Enter your 4-digit User Code

**DSC**

SECURITY SYSTEM QUICK REFERENCE GUIDE

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**WHEN TROUBLE LIGHT COMES ON**

• Press \* 2

• Keypad will describe the Trouble

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**TO SET TIME AND DATE**

• Press \* 6 and enter the 4-digit Master Code • 1 long beep indicates an error, press and enter the Master Code again • After 4 short beeps, press (1 then 10 digits, 2 each for the hour, minute, month, day and year (HH:MM MM/DD/YY)

- Use a 24-hour clock (e.g. 8:30 pm = 20:30) - Use 2 digits each to indicate the month and day (e.g. March 8 = 03 08) - Only enter the last 2 digits of any given year (e.g. 2007 = 07)

TO ENABLE DOOR CHIME FEATURE • Press and hold (Door Chime) for 2 seconds • 3 beeps = ON; 1 long beep = OFF

CHANGING KEYPAD BUZZER TONE • If using a PK5500 keypad, press \* 6 and enter the 4-digit Master Code then proceed with the following:

- Scroll to the phrase "Buzzer Control" and press \* • If using an LED or fixed-message keypad, press \* 6 and enter the 4-digit Master Code then proceed with the following:

- Press and hold (Left Arrow) - The tone will change - When the desired tone is identified, release (Left Arrow)

TO SOUND AN ALARM MANUALLY • Press and hold (Fire) or for 2 seconds

**DSC**